Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 34 - LIT-18626-12-89
P. 34

    UF4R10E0.book  Page 29  Tuesday, August 4, 2020  1:32 PM

                            Control function operation

                            EJU31273
                            Steering pole                         TIP:
                            The steering pole can be moved up or down   It will take about 60 seconds for the water
                            to change the height of the handlebars.  to reach the outlet after the engine is start-
                                                                   ed.
                                                                   Water  discharge may not be  constant
                                                                   when the engine is running at idling speed.
                                                                   If this occurs, apply a little throttle to make
                                                                   sure that water discharges properly.
                                                                  EJU40323
                                                                  Water separator
                                                                  The water separator prevents water from en-
                                                                  tering the fuel tank by collecting any water
                                                                  that has entered the fuel tank breather hose if
                                                                  the watercraft was capsized.
                            EJU35975                              If water has collected in the water separator,
                            Cooling water pilot outlet
                            When the engine  is running, some of  the  drain it by loosening the drain screw.
                            cooling water that is circulated in the engine
                            is discharged from  the cooling  water pilot    1
                            outlet.
                                                                            2

                                          1

                                                                   1 Water separator
                                                                   2 Drain screw
                                                                  To drain water from the water separator:
                              1 Cooling water pilot outlet        (1) Place a drain pan or dry cloth under the
                                                                     water separator.
                            There is a cooling water pilot outlet on the
                                                                  (2) Gradually loosen the drain screw to drain
                            port (left) side of the watercraft. To check for
                                                                     the water. Catch the draining water in the
                            proper operation of the cooling system, make
                                                                     drain pan or soak it up with the dry cloth
                            sure that water is being discharged from the
                                                                     so that it does not spill into the engine
                            cooling water pilot outlet. If water is not being
                                                                     compartment. If any water spills into the
                            discharged from the outlet, stop the engine
                                                                     watercraft, be sure to wipe it up with a
                            and check the jet intake for clogging. (See
                                                                     dry cloth.
                            page 78 for information on the jet intake.)
                                                                  (3) Securely tighten the drain screw until it
                                                                     stops.

                            29

| 29 30 31 32 33 34 35 36 37 38 39 |