Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-12-89
P. 56

    UF4R10E0.book  Page 51  Tuesday, August 4, 2020  1:32 PM

                            Pre-operation checks

                            pouch. Also, make  sure that the storage  EJU40122
                                                                  Safety equipment check
                            pouch is securely installed. (See page 35 for
                                                                  Check that safety equipment meeting the ap-
                            information on the storage pouch.)
                                                                  plicable regulations is on board.
                            EJU41082
                            Fire extinguisher holder, cover, and band   EJU32353
                                                                  Hull and deck check
                            checks                                Check the hull and deck for damage or other
                            Make sure that the fire extinguisher holder,
                                                                  problem.
                            cover, and band are not damaged and that
                                                                  EJU32657
                            the cover is securely held in place using the  Jet intake checks
                            band. (See page 36 for information on the fire  Make sure that the jet intake is not damaged
                            extinguisher holder, cover, and band.)  or clogged with weeds or debris. If the jet in-
                            EJU32535                              take is clogged, clean it. (See page 78 for in-
                            Fire extinguisher check               formation on the jet intake.)
                            Check that there is a full fire extinguisher on
                                                                  EJU44250
                            board.                                Stern drain plug checks
                                                                  Loosen the stern drain plugs and  remove
                                                                  them, and then make sure that the plugs and
                                                                  O-rings on the plugs are not damaged and
                                                                  that there is no foreign material on the
                                                                  threads or O-rings on  the plugs.  NOTICE:
                                                                  Before installing  the stern drain plugs,
                                                                  clean the  drain plug threads and the  O-
                                                                  rings on the plugs to remove any foreign
                                                                  materials, such as dirt or sand. Otherwise,
                                                                  the stern drain plugs could be damaged,
                            To check  the  fire extinguisher, see the  in-  allowing water to enter the engine com-
                            structions supplied  by the fire extinguisher  partment. Check the O-rings on the stern
                            manufacturer. Always keep the fire extin-  drain plugs and make sure that the plugs
                            guisher secured in the holder with its cover in  are tightened securely before launching
                            place.                                the  watercraft. Otherwise, water may
                            Always carry a fire extinguisher on board. A
                            fire extinguisher is not standard  equipment
                            with this watercraft. If you do not have one,
                            contact a Yamaha dealer or a fire extinguish-
                            er dealer to obtain one meeting the proper
                            specifications.
                              Fire extinguisher:
                                Classification:
                                  5-B (B-1)
                                Capacity:
                                  2 lb or more

                            51

| 51 52 53 54 55 56 57 58 59 60 61 |