Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 72 - LIT-18626-12-89
P. 72

    UF4R10E0.book  Page 67  Tuesday, August 4, 2020  1:32 PM

                            Care and storage

                                                                   Steering cable (jet thrust nozzle end) and
                              Recommended water-resistant grease:
                                YAMALUBE MARINE GREASE             ball joint

                             Throttle cable

                                                                  TIP:
                                                                  Disconnect the steering cable from the ball
                             Steering cable ball joint (handlebar end)  joint before lubricating.
                              and steering cable  inner wire (handlebar  EJU46021
                              end)                                Rustproofing
                                                                  ECJ01361

                                                                  Do not run  the engine for  more than 15
                                                                  seconds on land without supplying water,
                                                                  otherwise the engine could overheat.
                                                                  Spray metallic parts of the hull and engine
                                                                  with a rust inhibitor such as Yamalube Sili-
                                                                  cone Protectant & Lubricant.
                                                                  To rustproof the internal engine components:
                                                                  (1) Remove the hood. (See page 33 for hood
                            TIP:                                     removal and installation procedures.)
                            Disconnect the  steering cable (handlebar  (2) While loosening the clamp, remove the
                            end) from the ball joint before lubricating.  breather hose.
                                                                  (3) Make sure that the area around the wa-
                                                                     tercraft is clear, and then start the engine
                                                                     in a well-ventilated area.
                                                                  (4) Run the engine at a fast idle.
                                                                  (5) Quickly spray as much rust inhibitor as
                                                                     possible into the air intake duct through
                                                                     the breather hose joint. Use  Yamalube
                                                                     Stor-Rite Engine Fogging Oil or an equiv-
                                                                     alent. Keep spraying until the engine
                                                                     stalls (or a maximum of  15 seconds).
                                                                     WARNING! Do not pour or spray gaso-

                            67

| 67 68 69 70 71 72 73 74 75 76 77 |