Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - LIT-18626-12-89
P. 54

    UF4R10E0.book  Page 49  Tuesday, August 4, 2020  1:32 PM

                            Pre-operation checks

                            right and left fully turned positions of the jet  make sure that the steering pole does not
                            thrust nozzle.                        have any side play.

                                                                  EJU32595
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                              Difference between fully turned posi-
                              tions of jet thrust nozzle (distances A
                              and B):
                                Maximum 5 mm (0.20 in)
                            EJU32623
                            Steering pole check
                            Move the steering pole up and down several
                            times to make sure that operation is smooth
                            and unrestricted throughout the whole range,
                            and that the free play is not excessive. Also,

                            49

| 49 50 51 52 53 54 55 56 57 58 59 |