Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-89
P. 44

    UF4R10E0.book  Page 39  Tuesday, August 4, 2020  1:32 PM

                            Operation and handling requirements

                                                                  EJU40291
                              Fuel tank capacity:                     Engine oil requirements
                                19 L (5.0 US gal, 4.2 Imp.gal)
                                                                  EJU45590
                                                                  Engine oil
                                                                  ECJ00282

                                                                  Use only 4-stroke engine oil. Usage of 2-
                                                                  stroke engine oil could result in severe en-
                                                                  gine damage.

                                                                    Recommended engine oil:
                                                                      YAMALUBE 4W or 4-stroke motor oil
                                                                    Recommended engine oil type:
                                                                      SAE 10W-30, 10W-40, 20W-40,
                                                                      20W-50
                            (6) Stop filling when the fuel level just reach-  Recommended engine oil grade:
                                es the bottom of the filler tube. Do not fill  API SG, SH, SJ, SL
                                up the filler tube. Because fuel expands
                                when it heats up, heat from the engine or  Why Yamalube
                                                                  YAMALUBE oil is a Genuine YAMAHA Part
                                the sun can cause fuel to spill out of the
                                                                  born of the engineers’ passion and belief that
                                fuel tank. Do not leave the watercraft
                                                                  engine oil is an important liquid engine com-
                                with a full tank in direct sunlight.
                                                                  ponent. We form teams of specialists in the
                                                                  fields of mechanical engineering, chemistry,
                                                                  electronics and track testing, and have them
                                                1                 develop the engine together with the oil it will
                                                       2          use. Yamalube oils take full advantage of the
                                                                  base oil’s qualities and blend in the ideal ba-
                                                                  lance of additives to make sure the final oil
                                                                  clears our performance standards. Thus,
                                                                  Yamalube mineral, semisynthetic and syn-
                                                                  thetic oils have their own distinct characters
                              1 Fuel tank filler tube             and value. Yamaha’s experience gained over
                              2 Maximum fuel level                many  years of  research and development
                                                                  into oil  since the 1960’s  helps  make
                            (7) Wipe up any spilled fuel immediately with
                                                                  Yamalube the best choice for your Yamaha
                                a dry cloth.
                                                                  engine.
                            (8) Securely install the  hood in its original
                                position, and then install the fuel filler cap
                                by tightening it until it clicks.

                            39

| 39 40 41 42 43 44 45 46 47 48 49 |