Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-12-89
P. 51

    UF4R10E0.book  Page 46  Tuesday, August 4, 2020  1:32 PM

                                                                    Pre-operation checks

                                      ITEM                         ROUTINE                   PAGE
                             POST-LAUNCH CHECKS
                                                    Check that water is discharged from the cooling
                             Cooling water pilot outlet                                       52
                                                    water pilot outlet while the engine is running.
                                                    When the engine is started, check that the meter
                             Meter                  lighting comes on for a few seconds and then goes   52
                                                    off.
                            TIP:
                            To ensure safety and reliability, pre-operation checks should be made each time the water-
                            craft is used.

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |