Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 77 - LIT-18626-12-89
P. 77

    UF4R10E0.book  Page 72  Tuesday, August 4, 2020  1:32 PM

                                                                                 Maintenance

                            EJU43102
                            Periodic maintenance chart
                            The periodic maintenance chart gives general guidelines for periodic maintenance. Have a
                            Yamaha dealer perform the checks in the following chart. However, maintenance may need
                            to be performed more frequently depending on your operating conditions. If you have any
                            questions, consult a Yamaha dealer.
                            This “√” mark indicates items to be checked and serviced by a Yamaha dealer.
                                                                   Initial    Thereafter every
                                                                                   100    200
                                                                         50 hours
                                   Item             Operation              or 12   hours or  hours or   Page
                                                                  10 hours         12      24
                                                                          months   months  months
                                                                            *1
                                                                                   *1      *1
                                              Check fuel hoses and
                             Fuel line                                              √            —
                                              clamps
                             Fuel filler cap/Wa-  Check O-rings for cracks          √
                             ter separator    and deformation                                    —
                                              Check installation and
                             Fuel tank                                              √            —
                                              straps
                                              Check for clogs and dam-
                             Water inlet strainer                                   √            —
                                              age
                                              Check for damage and
                             Cooling water hos-  leakage, and check                 √            —
                             es
                                              clamps
                             Engine oil       Replace                √      √                    74
                             Oil filter       Replace                               √            74
                             Spark plugs      Check                  √              √            —
                                              Check state of charge,
                             Battery                                                √            —
                                              terminals and bands
                             Battery leads    Check terminals                       √            —
                             Steering master  Check and adjust       √              √            —
                                              Check exterior and con-
                             Steering cable                                         √            —
                                              nections, and lubricate
                                              Check for damage, and
                             Air intake hoses                                       √            —
                                              check clamps
                             Throttle body    Lubricate throttle valve              √            —
                                              Check for exhaust leak-
                             Exhaust system   age, and check hoses and              √            —
                                              clamps
                                              Check breather hose and
                             Breather hose                                          √            —
                                              clamps
                                              Check for bends, dam-
                             Impeller                                               √            —
                                              age, and foreign material
                                              Check movement, and lu-
                             Jet thrust nozzle                                      √            —
                                              bricate

                                                                                                   72

| 72 73 74 75 76 77 78 79 80 81 82 |