Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-12-89
P. 80

    UF4R10E0.book  Page 75  Tuesday, August 4, 2020  1:32 PM

                            Specifications

                            EJU45432                                Spark plug gap:
                                      Specifications                  0.7–0.8 mm (0.028–0.031 in)
                            Watercraft capacity:                    Battery capacity:
                              Maximum people on board:                12 V, 18 Ah
                                1 person                            Battery type:
                              Maximum load capacity:                  YTX20L-BS
                                80 kg (176 lb)                      Charging system:
                            Dimensions and weight:                    Flywheel magneto
                              Length:                             Drive unit:
                                2.43 m (95.7 in)                    Propulsion system:
                              Width:                                  Jet pump
                                0.76 m (29.9 in)                    Jet pump type:
                              Height:                                 Axial flow, single stage
                                0.79 m (31.1 in)                    Impeller rotation:
                              Dry weight:                             Counterclockwise
                                170 kg (375 lb)                     Jet thrust nozzle angle:
                            Performance:                              P1: 16.0+16.0°
                              Maximum fuel consumption:               P2: 19.0+19.0°
                                29.1 L/h (7.7 US gal/h, 6.4 Imp.gal/h)  Fuel and oil:
                              Cruising range at full throttle:      Recommended fuel:
                                0.65 hour                             Regular unleaded gasoline
                              Trolling speed:                       Minimum octane rating (PON):
                                1500 ±100 r/min                       86
                            Engine:                                 Minimum octane rating (RON):
                              Engine type:                            90
                                Liquid cooled 4-stroke, DOHC        Recommended engine oil:
                              Number of cylinders:                    YAMALUBE 4W or 4-stroke motor oil
                                3
                              Engine displacement:
                                1049 cm³
                              Bore × stroke:
                                82.0 × 66.2 mm (3.23 × 2.61 in)     Recommended engine oil type SAE:
                              Compression ratio:                      SAE 10W-30, 10W-40, 20W-40, 20W-50
                                11.0 : 1                            Recommended engine oil grade API:
                              Valve clearance-intake (cold):          API SG, SH, SJ, SL
                                0.15–0.22 mm (0.0059–0.0087 in)     Fuel tank total capacity:
                              Valve clearance-exhaust (cold):         19 L (5.0 US gal, 4.2 Imp.gal)
                                0.26–0.32 mm (0.0102–0.0126 in)     Engine oil quantity with oil filter replacement:
                              Lubrication system:                     3.4 L (3.59 US qt, 2.99 Imp.qt)
                                Dry sump                            Engine oil quantity without oil filter replacement:
                              Cooling system:                         3.2 L (3.38 US qt, 2.82 Imp.qt)
                                Water                               Engine oil total quantity:
                              Starting system:                        3.7 L (3.91 US qt, 3.26 Imp.qt)
                                Electric
                              Ignition system:
                                T.C.I.
                              Spark plug (NGK):
                                CR9EB

                            75

| 75 76 77 78 79 80 81 82 83 84 85 |