Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 20 - LIT-18626-12-89
P. 20

    UF4R10E0.book  Page 15  Tuesday, August 4, 2020  1:32 PM

                                Safety information

                            EJU30831                              EJU30871
                               Recommended equipment                    Hazard information
                            The following items  should be carried on   Never start the engine or let it run for any
                            board your watercraft:                 length of time in an enclosed area. Exhaust
                             Sound-signaling device               fumes contain carbon monoxide, a color-
                              You should carry a whistle or other sound-  less, odorless gas that may cause loss of
                              signaling device that can be used to signal  consciousness and death within a short
                              other boats. See “Rules of the Road” for  time. Always operate the watercraft in an
                              more information.                    open area.
                             Visual distress signals              Do not touch the hot oil tank, muffler, or en-
                              It is recommended that a U.S. Coast Guard  gine during or immediately after engine op-
                              approved pyrotechnic device be stored in a  eration; they can cause serious burns.
                              waterproof container on your watercraft. A
                              mirror can also be used as an emergency
                              signal. Contact a  Yamaha  dealer or the
                              U.S. Coast Guard for more information.
                             Watch
                              A watch is  helpful so you will know how
                              long you have been operating the water-
                              craft.
                             Towline
                              A towline can be used to tow a disabled
                              watercraft in an emergency.

                            15

| 15 16 17 18 19 20 21 22 23 24 25 |