Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 58 - LIT-18626-12-90
P. 58

    UF4P10E0.book  Page 52  Friday, July 31, 2020  8:50 AM

                            Instrument operation

                            TIP:                                  If a warning is activated, have the watercraft
                             While the engine overheat warning is acti-  serviced by a Yamaha dealer as soon as pos-
                              vated, the maximum engine speed is limit-  sible.
                              ed.                                 TIP:
                             Push the “OK” button of the touchpad con-  Push the “OK” button of the touchpad control
                              trol to display a description of the warning  to display a description of the warning in the
                              in the center display.              center display.
                            Oil pressure warning “  ”
                            If the oil pressure drops significantly, “  ”
                            and “  ” are shown in the warning bar, and
                            the buzzer sounds intermittently.

                            If the oil pressure warning is activated, imme-
                            diately reduce the engine  speed, return to
                            shore, and then check the engine oil level.
                            (See page 62 for information on checking the
                            engine oil level.) If the oil level is sufficient,
                            have a Yamaha dealer check the watercraft.
                            TIP:
                             While the oil pressure warning is activated,
                              the maximum engine speed is limited.
                             Push the “OK” button of the touchpad con-
                              trol to display a description of the warning
                              in the center display.
                            Other warnings (communication errors,
                            exceeding the maintenance intervals, and
                            so on) “  ”
                            If any other malfunction is detected or if the
                            engine has been operated for more than 50
                            hours since the last maintenance, the warn-
                            ing bar is shown instead of the tachometer
                            value display, “  ” is shown, and the buzz-
                            er sounds intermittently.

                            52

| 53 54 55 56 57 58 59 60 61 62 63 |