Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-90
P. 64

    UF4P10E0.book  Page 58  Friday, July 31, 2020  8:50 AM

                            Equipment operation

                            To open the seat storage compartment:  To close the seat storage compartment:
                            (1) Remove the rear seat. (See page 53 for  (1) Insert the projections on the lid into the
                                seat removal and installation proce-  slots on the seat storage compartment.
                                dures.)
                            (2) Push the latch forward, and then lift up
                                the lid and remove it.

                                         1
                                                             2

                                                                  (2) Push the rear of the lid down.

                              1 Lid
                              2 Latch

                                         1

                                                                  (3) Securely install the rear seat in its original
                                                                     position.
                                                                  EJU46030
                                                                  Fire extinguisher holder and cover
                              1 Seat storage compartment          The fire extinguisher holder and cover are lo-
                                                                  cated in the bow storage compartment.
                              Seat storage compartment:
                                Capacity:
                                  5.4 L (1.4 US gal, 1.2 Imp.gal)
                                Load limit:
                                  3.0 kg (7 lb)

                            58

| 59 60 61 62 63 64 65 66 67 68 69 |