Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 89 - LIT-18626-12-90
P. 89

    UF4P10E0.book  Page 83  Friday, July 31, 2020  8:50 AM

                                                                                      Operation

                            (2) Put one foot on the step, and then grasp  (6) Look  in all directions, start  the  engine,
                                the reboarding grip with your other hand.  and then start off slowly.
                                                                  EJU43260
                                                                  Boarding with passenger(s)
                                                                  EWJ01800

                                                                   Severe internal injuries can occur if wa-
                                                                   ter is forced into body cavities as a re-
                                                                   sult of being near the jet thrust nozzle.
                                                                   Do not start the engine until the passen-
                                                                   gers are  seated with  their feet on the
                                                                   floor of the footwell and are securely
                                                                   holding on to the person in front of them
                            (3) Pull yourself up onto the boarding plat-  or to the handgrip provided.
                                form and grasp the handgrip, and then   Before boarding the watercraft, make
                                move to the seat and sit astride.  sure that  the engine is  stopped. If the
                                                                   engine is running, the reverse gate may
                                                                   move  down  and a person boarding
                                                                   could be pinched.

                                                                  The heavier the total weight of the operator
                                                                  and passenger(s), the more difficult it will be
                                                                  to balance the watercraft. Do not operate the
                                                                  watercraft when the total weight exceeds 240
                                                                  kg (530 lb) including any cargo.
                                                                  To board with passenger(s):
                                                                  (1) Board as noted in the previous section
                            (4) Attach the engine shut-off cord (lanyard)
                                                                     “Boarding alone”.
                                to your left wrist, and then attach the clip
                                to the engine shut-off switch.
                            (5) Grip the handlebars with both hands and
                                place both feet on the floor of the foot-
                                well.

                                                                  (2) Grip the handlebars with both hands and
                                                                     place both feet on the floor of the foot-
                                                                     well.

                                                                                                   83

| 84 85 86 87 88 89 90 91 92 93 94 |