Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-90
P. 63

    UF4P10E0.book  Page 57  Friday, July 31, 2020  8:50 AM

                                                                     Equipment operation

                            To close the bow storage compartment:
                                                                    Glove compartment:
                            Push the rear of the hood down to securely  Capacity:
                            lock it in place.                           10.2 L (2.7 US gal, 2.2 Imp.gal)
                                                                      Load limit:
                                                                        1.5 kg (3 lb)

                                                                  To close the glove compartment:
                                                                  Push the lid down to securely lock it in place.

                            EJU46000
                            Glove compartment
                            The glove compartment is located in front of
                            the seat.
                            To open the glove compartment:
                            Push the glove compartment latch forward,  To drain water from the glove compartment:
                            and then lift up the lid.             (1) Remove the drain plug on the bottom of
                                                                     the glove compartment to drain the wa-
                                                                     ter.

                                                                                                  1
                                                     1

                              1 Glove compartment latch

                                                                   1 Drain plug
                                                                  (2) Securely install the drain plug in it original
                                                                     position.
                                                                  EJU46011
                                                                  Seat storage compartment
                                                          1       The seat storage compartment is located un-
                                                                  der the rear seat.
                                                                  The storage compartment is removable.

                              1 Glove compartment

                                                                                                   57

| 58 59 60 61 62 63 64 65 66 67 68 |