Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-12-90
P. 45

    UF4P10E0.book  Page 39  Friday, July 31, 2020  8:50 AM

                                                                      Watercraft operation

                            EJU40002                                 speed can be adjusted to two levels: +1
                              Watercraft operation modes
                                                                     and +2.
                            EJU45891
                            Reverse assist                                          1
                            The reverse assist is a function for temporar-
                            ily increasing the engine speed when moving
                            in  reverse,  such as to  enter the water
                            smoothly when launching the watercraft from
                                                                                   TRIM
                            a trailer.                                             T.D.E
                            This function operates after the  engine is
                            started and only if the watercraft is not shifted
                            into forward.
                                                                   1 RiDE lever
                            TIP:
                            Once the watercraft is shifted into forward af-
                            ter the engine is started, the reverse assist
                            cannot be operated.
                            Activating and deactivating the reverse
                            assist
                            The activation of  the reverse assist  can be
                            confirmed by the reverse assist indicator on
                            the multifunction information center.
                                                                                          1

                                                                   1 “SPEED ADJUST” switch
                                            RPM                   To deactivate the reverse assist:
                                            x1000
                                                                  Perform one of the following operations. The
                                                   MPH            beeper sounds two times and the reverse as-
                                       Reverse Assist  +2         sist indicator disappears when  the reverse
                                                                  assist is deactivated.
                              14.3V
                                                                   Relax your grip on the RiDE lever.
                                            1      2               Push  the lower side of the  “SPEED  AD-
                              1 Reverse assist indicator           JUST” switch when the reverse assist level
                              2 Reverse assist level               is set to +1.
                            To activate the reverse assist:        Squeeze the throttle lever.
                            (1) Start the engine.                 EJU45900
                                                                  T.D.E. (thrust directional enhancer)
                            (2) Squeeze the RiDE lever to the fully open
                                                                  The T.D.E. is a function for slightly lifting or
                                position, and then push the upper side of
                                                                  lowering the reverse gate from the neutral po-
                                the “SPEED ADJUST” switch. Once the
                                                                  sition to operate the watercraft at very low
                                beeper sounds three times and the re-
                                                                  speeds when the engine is running at idling
                                verse assist indicator is displayed,  the
                                                                  speed.
                                engine speed will increase. The engine
                                                                                                   39

| 40 41 42 43 44 45 46 47 48 49 50 |