Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 91 - LIT-18626-12-90
P. 91

    UF4P10E0.book  Page 85  Friday, July 31, 2020  8:50 AM

                                                                                      Operation

                              not  have brakes. Do  not release the  (2) Attach the engine shut-off cord (lanyard)
                              throttle lever when trying to steer away  to your left wrist, and then attach the clip
                              from objects—as with  other power-     to the engine shut-off switch.
                              boats, you need throttle to steer.  (3) Push the watercraft away from the dock,
                                                                     grip the handlebars with both hands, and
                            ECJ01341
                                                                     place both feet on the floor of the foot-
                                                                     well.
                            Never run the engine in water that is less
                            than 60 cm (2 ft) deep from the bottom of
                            the watercraft, otherwise pebbles or sand
                            could be sucked into the jet intake, caus-
                            ing impeller damage and engine overheat-
                            ing.

                                                                  (4) Look  in all directions, start  the  engine,
                                                                     and then start off slowly.
                                                                  EJU44210
                                                                  Capsized watercraft
                                                                  EWJ00672

                                                                  Improper uprighting can cause injury.
                            EJU45380
                            Starting off from a trailer            Be sure to shut the engine off by pulling
                            (1) Launch the watercraft.             on the engine shut-off cord (lanyard) to
                            (2) Attach the engine shut-off cord (lanyard)  remove the clip from the engine shut-off
                                to your left wrist, and then attach the clip  switch.
                                to the engine shut-off switch.     Do not put your hands in the intake
                            (3) Look in all directions, and then start the  grate.
                                engine.
                                                                  If the watercraft capsizes, turn it over imme-
                            (4) Squeeze the RiDE lever and  move the
                                                                  diately.
                                watercraft back slowly. (See page 35 for
                                                                  To upright the watercraft:
                                RiDE lever operation procedures.)
                                                                  (1) Remove the clip from the engine shut-off
                            TIP:                                     switch.
                            When using the RiDE lever to start off from a  (2) Swim to the rear of the watercraft. Turn
                            trailer, you can use the reverse assist to tem-  the watercraft over by pulling on the ride
                            porarily increase the engine speed. (See page  plate with one hand while pushing down
                            39 for reverse assist operation procedures.)
                            EJU33114
                            Boarding and starting off from a dock
                            (1) Board the watercraft from the side.

                                                                                                   85

| 86 87 88 89 90 91 92 93 94 95 96 |