Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 43 - LIT-18626-12-90
P. 43

    UF4P10E0.book  Page 37  Friday, July 31, 2020  8:50 AM

                                                                      Watercraft operation

                            TIP:                                  This function can be used only for  forward
                            If the RiDE lever is squeezed while the throttle  operation of the watercraft.
                            lever is squeezed, the  watercraft  will  slow  TIP:
                            down, and once stopped, move in reverse.   When the watercraft is moving in reverse or
                            To shift into neutral from forward:    is in neutral, the jet thrust nozzle will auto-
                            (1) Release the throttle lever.        matically change to the neutral trim setting.
                            (2) Lightly squeeze and release the RiDE le-  When the watercraft is shifted into forward,
                                ver. The “N” (neutral) shift indicator will  the  jet thrust nozzle will  automatically
                                be displayed.                      change to the selected trim setting.
                                                                   While the watercraft is in neutral,  the
                                                                   “TRIM/T.D.E.” switch controls the forward
                                                                   and reverse operation of the T.D.E. (thrust
                                                                   direction enhancer). (See page 39 for infor-
                                                                   mation on the T.D.E.)
                                                                   The watercraft performance characteristics
                                                                   according to the trim angle change de-
                                              TRIM
                                             T.D.E
                                                                   pending on the operating conditions.
                                                                  Confirming the trim setting
                                                                  The trim setting can be confirmed by the trim
                                                                  setting indicator on  the multifunction  infor-
                                                                  mation center.
                                                                      1
                                            RPM
                                            x1000
                                                   MPH
                                                                                 RPM
                                                                                 x1000
                              14.3V
                                                                                        MPH
                                                           1
                              1 “N” (Neutral position)
                                                                   14.3V
                            TIP:                                   1 Trim setting indicator
                            If the RiDE lever is squeezed continuously,
                                                                  To change the trim setting:
                            the reverse gate will move to the reverse po-
                                                                  (1) Shift into forward.
                            sition.
                                                                  (2) Push the upper side of the “TRIM/T.D.E.”
                            EJU45880
                            Electric trim system                     switch to  increase the trim  setting  and
                            The  electric trim system is a  function for  raise the bow, or push the lower side of
                            changing the vertical angle of the jet thrust  the “TRIM/T.D.E.” switch to decrease the
                            nozzle to change the trim angle and perfor-  trim setting and lower the bow. The trim
                            mance characteristics of the watercraft.

                                                                                                   37

| 38 39 40 41 42 43 44 45 46 47 48 |