Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-90
P. 50

    UF4P10E0.book  Page 44  Friday, July 31, 2020  8:50 AM

                            Watercraft operation

                                cruise assist indicator is displayed, the  changed in the range of the cruise assist
                                cruise assist is activated.          levels –5 to +5.

                                                        1                                 1
                              1 “CRUISE/NO WAKE” switch            1 “SPEED ADJUST” switch
                            (3) When the cruise assist is activated, slow-  TIP:
                                ly squeeze  the throttle  lever  to keep it  Because the cruise assist can only be set be-
                                squeezed further than  the position at  tween engine speeds of approximately 3000
                                which the cruise assist was set.  r/min and  approximately 7000 r/min, the
                            TIP:                                  cruise assist level cannot be adjusted to an
                            Check the multifunction information center to  engine speed outside of this range.
                            make sure that the cruise assist is activated  To deactivate the cruise assist:
                            before squeezing the throttle lever to the full  Relax your grip on the throttle lever past the
                            throttle position. If the cruise assist is not ac-  position at which the cruise assist was set.
                            tivated, the engine will respond normally to  The beeper sounds two times and the cruise
                            the throttle operation.               assist indicator disappears when the cruise
                            (4) Once the cruise assist is activated, push  assist is deactivated.
                                the upper side of the “SPEED ADJUST”
                                switch to increase the set engine speed
                                or  the lower side  of  the “SPEED AD-
                                JUST” switch to decrease the set engine
                                speed. The engine  speed can be

                            44

| 45 46 47 48 49 50 51 52 53 54 55 |