Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-90
P. 52

    UF4P10E0.book  Page 46  Friday, July 31, 2020  8:50 AM

                            Instrument operation

                            EJU45960                              (See page 50 for information about the warn-
                            Display
                                                                  ing descriptions.)
                            The display is configured as shown below.
                                                                          1                2
                                             1

                                                                                  RPM
                                                                                 x1000
                                            RPM
                                            x1000
                                                                                        MPH
                                                  MPH
                                                                     14.3V
                                14.3V
                                                                      3    4                   5
                                             2
                                                                   1 Trim setting indicator
                              1 Screen tab bar
                                                                   2 Fuel level meter
                              2 Center display
                                                                   3 Voltmeter
                                                                   4 Tachometer
                                                                   5 Shift indicator
                                                                  Trim setting indicator
                                                                  The position of  this indicator  indicates  the
                                             1                    trim setting of the jet thrust nozzle. (See page
                              1 Warning bar                       37 for information on the trim setting.)
                            Screen tab bar                        Voltmeter
                            When each symbol is selected, the watercraft  The voltmeter shows the battery voltage.
                            information, function settings, and other in-  When the battery voltage is normal, the volt-
                            formation are shown  in the center display.  meter displays approximately 14 volts.
                            (See page 47 for information on each screen.)  If the battery voltage has dropped or  risen
                            Center display                        significantly, the battery voltage warning will
                            The center display shows the watercraft in-  activate and the voltage display will blink.
                            formation, function settings, and other infor-  (See page 51 for information on the battery
                            mation  according  to the symbol on the  voltage warning.)
                            screen tab bar that is selected.      Tachometer
                            Warning bar                           The tachometer shows the engine speed us-
                            The warning bar is shown when an error or  ing the numbers ×1000 RPM (r/min) and the
                            malfunction is detected.              number of display segments.
                            Push the “OK” button of the touchpad control  Shift indicator
                            when  the warning symbol is displayed  to  This indicator shows the  reverse  gate shift
                            show  the warning description,  error code,  positions: “F” (forward), “N” (neutral), and “R”
                            and other information in the center display.  (reverse).  (See page 35 for shifting proce-
                                                                  dures.)

                            46

| 47 48 49 50 51 52 53 54 55 56 57 |