Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-91
P. 42

    UF4M10E0.book  Page 36  Tuesday, August 4, 2020  11:35 AM

                            Watercraft operation

                            and the “N” (neutral) shift indicator will be dis-  To shift into forward:
                            played.                               (1) Release the RiDE lever.
                                                                  (2) Squeeze the throttle lever. The reverse
                                          1                          gate  will rise completely, the engine
                                                                     speed will increase, the watercraft will
                                                                     start moving forward, and the “F” (for-
                                                                     ward) shift indicator will be displayed.

                                                                                1
                                              TRIM
                                             T.D.E

                              1 RiDE lever

                                                 1

                                                                   1 Throttle lever

                                                                                 1
                                                             2

                                                                                                 2
                              1 Reverse gate
                              2 Neutral position

                                            RPM                    1 Reverse gate
                                            x1000
                                                                   2 Forward position
                                                   MPH

                              14.3V                                              RPM
                                                                                 x1000
                                                           1
                              1 “N” (Neutral position)                                  MPH
                            TIP:
                            Although the neutral position helps keep the  14.3V
                            watercraft from moving even when the en-                            1
                            gine is running, some movement may occur.
                                                                   1 “F” (Forward position)

                            36

| 37 38 39 40 41 42 43 44 45 46 47 |