Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 88 - LIT-18626-12-91
P. 88

    UF4M10E0.book  Page 82  Tuesday, August 4, 2020  11:35 AM

                            Operation

                            current location. (See page 35 for shift sys-  bles or sand could be sucked into the jet
                            tem operation procedures.)            intake, causing impeller damage and en-
                                                                  gine overheating. [ECJ00473]

                                            RPM
                                            x1000
                                                   MPH
                                                                               60 cm (2 ft)
                              14.3V
                                                           1
                              1 “N” (Neutral position)
                                                                  EJU42461
                                                                  Boarding alone
                                                                  (1) From the rear of the watercraft, lower the
                                                                     reboarding step with one hand and hold
                                                                     it in place.

                            EJU42451
                            Boarding the watercraft
                            EWJ01112

                            Be sure the operator and any passengers
                            have practiced  boarding from the water  (2) Put one foot on the step, and then grasp
                            while still close to shore before riding. A  the reboarding grip with your other hand.
                            person who has made many unsuccessful
                            attempts to get back on  the watercraft
                            may become fatigued and suffer from ex-
                            posure, increasing the risk of injury and
                            drowning.
                            Board the watercraft  in water free from
                            weeds and debris and at least 60 cm (2 ft)
                            deep  from the  bottom of the watercraft.
                            NOTICE: Never run the engine in water
                            that is less than 60 cm (2 ft) deep from the
                            bottom of the watercraft, otherwise peb-

                            82

| 83 84 85 86 87 88 89 90 91 92 93 |