Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-91
P. 46

    UF4M10E0.book  Page 40  Tuesday, August 4, 2020  11:35 AM

                            Watercraft operation

                            This function can be used only when the wa-  “TRIM/T.D.E.” switch to move in reverse
                            tercraft is in neutral.                  at a very low speed.
                            TIP:
                            While the watercraft is shifted into forward,
                            the “TRIM/T.D.E.” switch controls the electric
                            trim system. (See page 37 for information on
                            the electric trim system.)
                            Activating and deactivating the T.D.E.
                            The activation of the T.D.E. can be confirmed
                            by the T.D.E. indicator on the multifunction     1
                            information center.
                                         2    T.D.E. FORWARD       1 “TRIM/T.D.E.” switch
                                         3    T.D.E. REVERSE      TIP:
                                            RPM
                                            x1000                 While the T.D.E. is activated, the “N” (neutral)
                                                                  shift indicator will be displayed and “0” will be
                                                   MPH
                                                                  displayed on the speedometer.
                                       T.D.E. FORWARD             To deactivate the T.D.E.:
                                                                  Perform one of the following operations. The
                              14.3V
                                                                  T.D.E. indicator disappears and the T.D.E. is
                                             1                    deactivated.
                              1 T.D.E. indicator
                                                                   Squeeze the throttle lever.
                              2 Forward operation at a very low speed
                                                                   Squeeze the RiDE lever.
                              3 Reverse operation at a very low speed
                                                                   Push  and hold the “CRUISE/NO  WAKE”
                            To activate the T.D.E.:                switch.
                            (1) Shift into neutral.                While moving forward at a very low speed,
                            (2) Push the upper side of the “TRIM/T.D.E.”  push the lower side of the “TRIM/T.D.E.”
                                switch to move forward at  a very low  switch.
                                speed or push the lower side of the   While moving in reverse at a very low
                                                                   speed, push the  upper side of  the
                                                                   “TRIM/T.D.E.” switch.
                                                                  TIP:
                                                                  The T.D.E. is also deactivated when the en-
                                                                  gine is stopped.
                                                                  EJU45910
                                                                  No-wake mode
                                                                  The no-wake mode is a function that main-
                                                                  tains the engine speed at a fixed setting for
                                                                  operating the watercraft at low speeds. While
                                                                  the watercraft is operating in no-wake mode,
                                                                  the engine speed can be adjusted to one en-

                            40

| 41 42 43 44 45 46 47 48 49 50 51 |