Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 97 - LIT-18626-12-91
P. 97

    UF4M10E0.book  Page 91  Tuesday, August 4, 2020  11:35 AM

                                                                           Care and storage

                                                                  EJU33493
                              Recommended water-resistant grease:        Long-term storage
                                YAMALUBE MARINE GREASE
                                                                  EWJ00331
                            (4) Store  the battery in a cool,  dry  place.
                                                                  Always place the watercraft upright in a
                                NOTICE: Storing the battery in an un-
                                                                  horizontal position when storing it, other-
                                charged condition can cause perma-
                                                                  wise fuel could leak out into the engine or
                                nent battery damage. Check the
                                                                  engine compartment, which could create
                                battery periodically. [ECJ00103]
                                                                  a fire hazard.
                            To install the battery:
                            (1) Place the battery in the battery compart-  Storage for long periods of time, such as win-
                                ment and hook the battery bands onto  ter storage, requires preventive maintenance
                                the holders.                      to ensure against deterioration. It is advisable
                            (2) Connect the positive (+) battery lead (red)  to have the watercraft serviced by a Yamaha
                                to the  positive (+) battery terminal.  dealer prior to storage.
                                NOTICE: Reversal of the battery leads  However, the following procedures can be
                                will damage the electrical parts. [ECJ00262]  performed easily by the owner.
                            (3) Connect the  negative (–)  battery lead  EJU40256
                                                                  Cleaning
                                (black) to the negative (–) battery termi-
                                                                  (1) Flush the cooling water passages. (See
                                nal.
                                                                     page 88 for information on flushing the
                            (4) Make sure that the battery is securely
                                                                     cooling water passages.)
                                held in place.
                                                                  TIP:
                                                                  If you will be storing the watercraft for a pro-
                                                                  longed period, such as winter storage, top off
                                                                  the fuel tank with fresh gasoline and add one
                                                                  ounce of Yamalube Fuel Stabilizer & Condi-
                                                                  tioner Plus to each gallon of fuel in the fuel
                                                                  tank before starting the engine.
                                                                  (2) Clean the watercraft. (See page 89 for in-
                                                                     formation on cleaning the watercraft.)
                                                                     Wax the  hull with a non-abrasive wax
                                                                     such as Yamalube Professional Polish.
                                                                  EJU44950
                                                                  Lubrication
                                                                  To keep moving parts sliding or rotating
                                                                  smoothly, lubricate them with water-resistant
                                                                  grease.
                                                                    Recommended water-resistant grease:
                                                                      YAMALUBE MARINE GREASE

                                                                                                   91

| 92 93 94 95 96 97 98 99 100 101 102 |