Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - LIT-18626-12-91
P. 37

    UF4M10E0.book  Page 31  Tuesday, August 4, 2020  11:35 AM

                                                             Control function operation

                            than 15 seconds without supplying water,  EJU31164
                                                                  Engine shut-off switch “  ”
                            otherwise the engine could overheat.
                                                                  The engine  shut-off switch  automatically
                            The  engine start/stop switch  (red button)  stops the engine when the clip, on the end of
                            starts the engine when the switch is pushed  the engine shut-off cord (lanyard), is removed
                            while the engine is stopped, and stops the  from the switch, such as if the operator falls
                            engine when the switch is pushed while the  off the watercraft.
                            engine is running.                    Insert the clip  under  the engine  shut-off
                            Release the engine start/stop switch as soon  switch before starting the engine.
                            as the engine starts to run. If the engine does
                            not start in 5 seconds, release the engine                         1
                            start/stop switch, wait 15 seconds, and then
                            try again. NOTICE: Never push the engine
                            start/stop switch while the engine is run-
                            ning. Do not operate the engine start/stop
                            switch for more than 5 seconds, otherwise
                            the battery will be discharged and the en-                          2
                            gine will not start. Also, the starter motor
                                                                                              3
                            could be damaged. [ECJ02860]
                                                                   1 Engine shut-off switch
                                                                   2 Clip
                                                                   3 Engine shut-off cord (lanyard)
                                                                  When the engine is not running, remove the
                                                                  clip from the engine shut-off switch to pre-
                                                                  vent accidental starting or unauthorized op-
                                                                  eration by children or others.

                                                 1

                              1 Engine start/stop switch
                            The engine will not start under any of the fol-
                            lowing conditions:
                             Lock mode of the Yamaha Security System
                              has been  selected. (See page 30 for
                              Yamaha Security System setting proce-
                              dures.)
                             Clip is removed  from  the engine  shut-off
                              switch.
                             Throttle lever is squeezed.
                             Throttle lever is malfunctioning.
                             RiDE lever is squeezed.
                             RiDE lever is malfunctioning.

                                                                                                   31

| 32 33 34 35 36 37 38 39 40 41 42 |