Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 81 - LIT-18626-12-91
P. 81

    UF4M10E0.book  Page 75  Tuesday, August 4, 2020  11:35 AM

                                                                    Pre-operation checks

                            EJU40553                              safe distance away from people, objects,
                            Cooling water pilot outlet check
                            Make sure that water is discharged from the  and other watercraft. [EWJ01860]
                            cooling water pilot outlet while the engine is
                            running. (See page 33 for information on the
                            cooling water pilot outlet.)                         RPM
                                                                                 x1000

                                                                                        MPH
                                                                                         2
                                                                                         3
                                                                   14.3V
                                                                                         4
                                                                                                1
                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                            EJU45260                              EJU40172
                            Multifunction information center check  Engine idling speed check
                            Make sure that the multifunction information  Start the engine and warm it up. Use the ta-
                            center operates properly. (See page 45 for in-  chometer in the multifunction  information
                            formation on proper operation of the multi-  center to make sure  that the engine  idling
                            function information center.)         speed is not significantly above or below the
                            EJU43392
                            Shift system check                    specified range.
                            Operate the throttle lever and RiDE lever, and
                                                                    Engine idling speed:
                            check that the watercraft moves or does not  1300 ±100 r/min
                            move according to the displayed shift indica-
                            tor. (See page 35 for shift system operation
                            procedures.)  WARNING! To avoid colli-
                            sions, operate at safe speeds and keep a

                                                                                                   75

| 76 77 78 79 80 81 82 83 84 85 86 |