Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-91
P. 39

    UF4M10E0.book  Page 33  Tuesday, August 4, 2020  11:35 AM

                                                             Control function operation

                            To adjust the handlebar position:     (2) Make sure that the tilt lever returns to its
                            (1) Pull the tilt lever up to disengage the han-  original position and that the handlebars
                                dlebar lock, and then move the handle-  are securely locked in place.
                                bars back or forth to the desired position.
                                WARNING! Never pull the tilt lever dur-
                                ing  operation, otherwise the  handle-
                                bars may  suddenly change  position,
                                which may lead to an accident. [EWJ00042]

                                                      1
                                                                  EJU35975
                                                                  Cooling water pilot outlet
                                                                  When the engine  is running, some of the
                                                                  cooling water that is circulated in the engine
                                                                  is discharged from  the cooling  water pilot
                              1 Tilt lever                        outlet.

                                                                            1
                                                                   1 Cooling water pilot outlet
                                                                  There is a cooling water pilot outlet on the
                                                                  port (left) side of the watercraft. To check for
                                                                  proper operation of the cooling system, make
                                                                  sure that water is being discharged from the
                                                                  cooling water pilot outlet. If water is not being
                                                                  discharged from the outlet, stop the engine
                                                                  and check the jet intake for clogging. (See
                                                                  page 102 for information on the jet intake.)

                                                                                                   33

| 34 35 36 37 38 39 40 41 42 43 44 |