Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 60 - LIT-18626-12-92
P. 60

    UF4S10E0.book  Page 54  Monday, September 28, 2020  1:50 PM

                            Equipment operation

                            could fall, which could result in severe in-  The storage compartments are not designed
                            jury. [EWJ01511]                      to be waterproof.  If you carry objects that
                                                                  must be kept dry, put them in a waterproof
                                                                  bag.
                                                                  Make sure  that the storage  compartments
                                                         1
                                                                  are closed securely before operating the wa-
                                                                  tercraft.
                                                                  EJU45250
                                                                  Bow storage compartment
                                                                  The bow storage compartment is located un-
                                                                  der the hood.
                                                                  To open the bow storage compartment:
                                                                  Pull the hood latch rearward, and then lift up
                              1 Cleat
                                                                  the rear of the hood.
                            EJU34894
                            Pull-up cleats
                            The pull-up cleats are used to attach a rope                         1
                            to the watercraft when mooring it.
                            To use a pull-up cleat, pull it up. The pull-up
                            cleat returns automatically to its original posi-
                            tion when released. WARNING! Do not use
                            the pull-up cleats to lift the watercraft. The
                            pull-up cleats are not designed to support
                            the watercraft’s weight. If the pull-up
                            cleats break, the watercraft could fall,
                                                                   1 Hood latch
                            which could result in severe injury. [EWJ00822]

                                                           1                       1

                                       2

                                                                   1 Bow storage compartment
                              1 Pull-up cleat
                              2 Pull-up cleat (VX LIMITED HO)       Bow storage compartment:
                                                                      Capacity:
                            EJU31685
                            Storage compartments                        92.0 L (24.3 US gal, 20.2 Imp.gal)
                                                                      Load limit:
                            This watercraft is equipped with the following
                                                                        5.0 kg (11 lb)
                            storage compartments.

                            54

| 55 56 57 58 59 60 61 62 63 64 65 |