Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 77 - LIT-18626-12-92
P. 77

    UF4S10E0.book  Page 71  Monday, September 28, 2020  1:50 PM

                                                                    Pre-operation checks

                            falls off, allowing the watercraft to conti-  (See page 30 for information on operating
                            nue to run and cause an accident. [EWJ01221]  each switch.)
                                                                                    1
                                                                                                2

                                                                                              3
                                                                   1 Clip
                            EJU46050
                            Switch checks                          2 Engine shut-off switch
                            ECJ01311
                                                                   3 Engine shut-off cord (lanyard)
                            Do not run the engine over 4000 r/min on
                            land. Also, do not run the engine for more
                            than 15 seconds without supplying water,
                            otherwise the engine could overheat.

                            Check the engine start/stop switch and the
                            engine shut-off switch for proper operation.

                                                                                      1
                                                                   1 Engine start/stop switch
                                                                  To check the operation of the switches:
                                                                  (1) If the lock mode is selected for the
                                                                     Yamaha Security System setting, select
                                                                     the unlock mode. (See  page 30 for
                                                                     Yamaha Security System setting proce-
                                                                     dures.)
                                                                  (2) Push the engine start/stop switch  to
                                                                     make sure that the engine starts.
                                                                  (3) As  soon as the  engine starts running,
                                                                     push  the engine start/stop switch to
                                                                     make sure that the engine stops immedi-
                                                                     ately.
                                                                  (4) Restart the engine, and then pull the en-
                                                                     gine  shut-off cord (lanyard) to  remove
                                                                     the clip from the engine shut-off switch

                                                                                                   71

| 72 73 74 75 76 77 78 79 80 81 82 |