Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - LIT-18626-12-92
P. 37

    UF4S10E0.book  Page 31  Monday, September 28, 2020  1:50 PM

                                                             Control function operation

                            than 15 seconds without supplying water,  from the switch, such as if the operator falls
                            otherwise the engine could overheat.  off the watercraft.
                                                                  Insert the clip  under  the engine  shut-off
                            The  engine start/stop switch  (red button)
                                                                  switch before starting the engine.
                            starts the engine when the switch is pushed
                            while the engine is stopped, and stops the
                            engine when the switch is pushed while the                         1
                            engine is running.
                            Release the engine start/stop switch as soon
                            as the engine starts to run. If the engine does
                            not start in 5 seconds, release the engine
                            start/stop switch, wait 15 seconds, and then                        2
                            try again.
                                                                                              3
                                                                   1 Engine shut-off switch
                                                                   2 Clip
                                                                   3 Engine shut-off cord (lanyard)
                                                                  When the engine is not running, remove the
                                                                  clip from the engine shut-off switch to pre-
                                                                  vent accidental starting or unauthorized op-
                                                                  eration by children or others.
                                                 1

                              1 Engine start/stop switch
                            The engine will not start under any of the fol-
                            lowing conditions:
                             Lock mode of the Yamaha Security System
                              has been  selected. (See page 30 for
                              Yamaha Security System setting proce-
                              dures.)
                             Clip is removed  from  the engine  shut-off
                              switch.
                             Throttle lever is squeezed.
                             Throttle lever is malfunctioning.
                             RiDE lever is squeezed.
                             RiDE lever is malfunctioning.
                            EJU31164
                            Engine shut-off switch “  ”
                            The  engine shut-off switch  automatically
                            stops the engine when the clip, on the end of
                            the engine shut-off cord (lanyard), is removed

                                                                                                   31

| 32 33 34 35 36 37 38 39 40 41 42 |