Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 61 - LIT-18626-12-92
P. 61

    UF4S10E0.book  Page 55  Monday, September 28, 2020  1:50 PM

                                                                     Equipment operation

                            To close the bow storage compartment:  To open the glove compartment:
                            Push the rear of the hood down to securely  Pull the glove compartment latch  up,  and
                            lock it in place.                     then lift up the lid.

                                                                                              1

                                                                   1 Glove compartment latch
                            EJU46211
                            Glove compartment
                            The glove compartment is located in front of
                            the seat.
                            TIP:
                             Make sure the seal of lid is intact, clear and
                              properly positioned before using.                           1
                             Make sure the seals around the USB char-
                              ger and 12V DC outlet are intact and prop-
                              erly positioned before using.
                             Completely  dry inside of the glove com-
                              partment and its contents before and after  1 Glove compartment
                              using.
                                                                    Glove compartment:
                             Make sure nothing is pinches between the
                                                                      Capacity:
                              glove compartment and the lid when clos-  16.5 L (4.4 US gal, 3.6 Imp.gal)
                              ing the glove compartment.              Load limit:
                             When not in use, the rubber caps for the  1.5 kg (3 lb)
                              USB charger and 12V DC outlet should be
                              installed to cover the connectors.

                                                                                                   55

| 56 57 58 59 60 61 62 63 64 65 66 |