Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 43 - LIT-18626-12-92
P. 43

    UF4S10E0.book  Page 37  Monday, September 28, 2020  1:50 PM

                                                                      Watercraft operation

                                speed can be adjusted to two levels: +1  This function can be used only when the wa-
                                and +2.                           tercraft is in neutral.
                                                                  Activating and deactivating the T.D.E.
                                                                  The activation of the T.D.E. can be confirmed
                                              1
                                                                  by the T.D.E. indicator on the multifunction
                                                                  information center.

                                                                               2   T.D.E. FORWARD
                                                                               3   T.D.E. REVERSE
                                                                                         MPH
                                                                                         RPM
                              1 RiDE lever                                   T.D.E. FORWARD

                                                                   14.3V
                                                                                   1
                                                                   1 T.D.E. indicator
                                                                   2 Forward operation at a very low speed
                                                                   3 Reverse operation at a very low speed
                                                                  To activate the T.D.E.:
                                                                  (1) Shift into neutral.
                                                    1             (2) Push the  upper side of  the “T.D.E.”
                                                                     switch to move forward at a very  low
                              1 “SPEED ADJUST” switch                speed or push the lower side of the
                                                                     “T.D.E.” switch to move in reverse at a
                            To deactivate the reverse assist:
                                                                     very low speed.
                            Perform one of the following operations. The
                            beeper sounds two times and the reverse as-
                            sist indicator  disappears when the  reverse
                            assist is deactivated.
                             Relax your grip on the RiDE lever.
                             Push the lower side of the “SPEED AD-
                              JUST” switch when the reverse assist level
                              is set to +1.
                             Squeeze the throttle lever.
                                                                             1
                            EJU46280
                            T.D.E. (thrust directional enhancer)
                            The T.D.E. is a function for slightly lifting or  1 “T.D.E.” switch
                            lowering the reverse gate from the neutral po-
                                                                  TIP:
                            sition  to  operate the watercraft at  very low
                                                                  While the T.D.E. is activated, the “N” (neutral)
                            speeds when the engine is running at idling
                                                                  shift indicator will be displayed and “0” will be
                            speed.
                                                                  displayed on the speedometer.

                                                                                                   37

| 38 39 40 41 42 43 44 45 46 47 48 |