Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-92
P. 39

    UF4S10E0.book  Page 33  Monday, September 28, 2020  1:50 PM

                                                             Control function operation

                            is discharged from  the cooling  water pilot  If water has collected in the water separator,
                            outlet.                               drain it by loosening the drain screw.

                                                                                                   1
                                                                                                   2

                                    1
                              1 Cooling water pilot outlet         1 Water separator
                            There is a cooling water pilot outlet on the  2 Drain screw
                            port (left) side of the watercraft. To check for  To drain water from the water separator:
                            proper operation of the cooling system, make  (1) Place a drain pan or dry cloth under the
                            sure that water is being discharged from the  water separator.
                            cooling water pilot outlet. If water is not being  (2) Gradually loosen the drain screw to drain
                            discharged from the outlet, stop the engine  the water. Catch the draining water in the
                            and check the jet intake for clogging. (See  drain pan or soak it up with the dry cloth
                            page 101 for information on the jet intake.)  so that it does not spill into the engine
                            TIP:                                     compartment. If any water spills into the
                                                                     watercraft, be sure to wipe it up with a
                             It will take about 60 seconds for the water
                                                                     dry cloth.
                              to reach the outlet after the engine is start-
                                                                  (3) Securely tighten the drain screw until it
                              ed.
                                                                     stops.
                             Water discharge may not  be  constant
                              when the engine is running at idling speed.
                              If this occurs, apply a little throttle to make
                              sure that water discharges properly.
                            EJU40323
                            Water separator
                            The water separator prevents water from en-
                            tering the fuel tank by collecting any water
                            that has entered the fuel tank breather hose if
                            the watercraft was capsized.

                                                                                                   33

| 34 35 36 37 38 39 40 41 42 43 44 |