Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-92
P. 49

    UF4S10E0.book  Page 43  Monday, September 28, 2020  1:50 PM

                                                                     Instrument operation

                            EJU46290                              (See page 47 for information about the warn-
                            Display
                                                                  ing descriptions.)
                            The display is configured as shown below.
                                                                                               1
                                                         1

                                                                                        MPH
                                                   MPH
                                                                                        RPM
                                                   RPM
                                                                     14.3V
                                14.3V
                                                                      2            3           4
                                             2
                                                                   1 Fuel level meter
                              1 Screen tab bar
                                                                   2 Voltmeter
                              2 Center display
                                                                   3 Tachometer
                                                                   4 Shift indicator
                                                                  Voltmeter
                                                                  The voltmeter shows the battery voltage.
                                                                  When the battery voltage is normal, the volt-
                                             1                    meter displays approximately 14 volts.
                              1 Warning bar                       If the battery voltage has dropped or  risen
                            Screen tab bar                        significantly, the battery voltage warning will
                            When each symbol is selected, the watercraft  activate and the voltage display will blink.
                            information, function settings, and other in-  (See page 47 for information on the battery
                            formation are shown  in the center display.  voltage warning.)
                            (See page 44 for information on each screen.)  Tachometer
                            Center display                        The tachometer shows the engine speed and
                            The center display shows the watercraft in-  the number of display segments.
                            formation, function settings, and other infor-  Shift indicator
                            mation  according  to the symbol on the  This indicator shows the  reverse  gate shift
                            screen tab bar that is selected.      positions: “F” (forward), “N” (neutral), and “R”
                            Warning bar                           (reverse).  (See page 34 for shifting proce-
                            The warning bar is shown when an error or  dures.)
                            malfunction is detected.              Fuel level meter
                            Push the “OK” button of the touchpad control  The fuel level meter shows the amount of fuel
                            when  the warning symbol is displayed  to  remaining in the fuel tank using the number of
                            show  the warning description,  error code,  display segments.
                            and other information in the center display.  If the amount of remaining fuel is low, the fuel
                                                                  level warning will activate. (See page 47 for
                                                                  information on the fuel level warning.)

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |