Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-12-92
P. 62

    UF4S10E0.book  Page 56  Monday, September 28, 2020  1:50 PM

                            Equipment operation

                            To close the glove compartment:       (2) Push the latch forward, and then lift up
                            Push the lid down to securely lock it in place.  the lid and remove it.

                                                                                 1
                                                                                                  2

                            To drain water from the glove compartment:  1 Lid
                                                                   2 Latch
                            (1) Remove the drain plug on the bottom of
                                the glove compartment to drain the wa-
                                ter.                                                      1

                                                             1

                                                                   1 Seat storage compartment
                                                                    Seat storage compartment:
                              1 Drain plug
                                                                      Capacity:
                            (2) Securely install the drain plug in it original  5.4 L (1.4 US gal, 1.2 Imp.gal)
                                                                      Load limit:
                                position.
                                                                        3.0 kg (7 lb)
                            EJU46011
                            Seat storage compartment
                            The seat storage compartment is located un-
                            der the rear seat.
                            The storage compartment is removable.
                            To open the seat storage compartment:
                            (1) Remove the rear seat. (See page 51 for
                                seat removal and installation proce-
                                dures.)

                            56

| 57 58 59 60 61 62 63 64 65 66 67 |