Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-92
P. 46

    UF4S10E0.book  Page 40  Monday, September 28, 2020  1:50 PM

                            Watercraft operation

                            (2) Select the maximum  watercraft  speed  (3) Select “Lock”.
                                setting under “Speed” and the accelera-  EJU45930
                                                                  Cruise assist
                                tion setting under “Accel.”
                                                                  The cruise assist is a function for maintaining
                                     1                2           a desired engine speed within a fixed range
                                                                  while operating the watercraft. Once the
                                         Drive Control
                                   Speed            Accel.        cruise assist is  activated, the  set  engine
                                                                  speed can be increased or decreased. How-
                                    High
                                                    Nomal
                                                                  ever, the adjustment is limited to a maximum
                                   Middle
                                                                  of five increments above or below the initial
                                                     Slow
                                    Low
                                                                  cruise assist setting.
                                            Save
                                                                  TIP:
                                             3                    The cruise assist can only be set between en-
                              1 Maximum watercraft speed setting  gine speeds of approximately 3000 r/min and
                              2 Acceleration setting              approximately 7000 r/min.
                              3 “Save”                            Activating and deactivating the cruise as-
                            (3) Select the “Save” button to complete the  sist
                                settings and return to the previous dis-  Activation of the cruise assist can be con-
                                play.                             firmed by the cruise assist indicator on the
                            Locking the drive control mode        multifunction information center.
                            The drive control mode can be locked.
                            To lock the drive control mode:
                            (1) Select “Lock”.
                            (2) Input each digit of the 4-digit PIN, and                 MPH
                                then push the “OK” button of the touch-
                                pad control.                                             RPM
                                                                             Cruise Assist  +4
                                                                   14.3V
                                          Enter PIN
                                                                                 1      2
                                          * * * *
                                     1       2       3             1 Cruise assist indicator
                                                                   2 Cruise assist level
                                     4       5       6
                                                                  To activate the cruise assist:
                                     7       8       9
                                                                  (1) Operate the throttle lever until the de-
                                             0
                                                                     sired engine speed is reached.
                                                                  (2) When the engine speed reaches the de-
                                                                     sired cruise assist  setting, push  the
                            To unlock the drive control mode:
                                                                     “CRUISE/NO WAKE” switch. Once  the
                            (1) Select the drive control mode indicator.
                                                                     beeper sounds three times and the
                            (2) Input each digit of the 4-digit PIN, and
                                then push the “OK” button of the touch-
                                pad control.

                            40

| 41 42 43 44 45 46 47 48 49 50 51 |