Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-12-92
P. 56

    UF4S10E0.book  Page 50  Monday, September 28, 2020  1:50 PM

                            Instrument operation

                            Cursor button “ / ”                   EJU46330
                            Press these buttons to adjust the volume.  USB charger
                                                                  There  is a USB  charger located inside  the
                            To connect an external device:
                                                                  glove compartment. The USB charger can be
                            (1) Turn on the Bluetooth function of the ex-
                                                                  used to charge external devices.
                                ternal device,  and then  search for  this
                                audio system.
                            (2) Turn the audio system on by pushing the
                                power button on the audio control.
                            (3) Select this audio system to connect to it.                       1
                            To disconnect an external device:
                            Turn the Bluetooth function of the external
                            device off.
                            EJU46320
                            Accessory outlet
                            There is a 12 V DC outlet located inside the
                            glove compartment. NOTICE: Do not use an  1 USB charger
                            automotive cigarette lighter or other ac-
                            cessories that get hot because the outlet
                            can be damaged. [ECJ02880]

                               1

                              1 12V DC outlet

                            50

| 51 52 53 54 55 56 57 58 59 60 61 |