Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 90 - LIT-18626-12-92
P. 90

    UF4S10E0.book  Page 84  Monday, September 28, 2020  1:50 PM

                            Operation

                              from objects—as with  other power-  (2) Attach the engine shut-off cord (lanyard)
                              boats, you need throttle to steer.     to your left wrist, and then attach the clip
                                                                     to the engine shut-off switch.
                            ECJ01341
                                                                  (3) Push the watercraft away from the dock,
                                                                     grip the handlebars with both hands, and
                            Never run the engine in water that is less
                                                                     place both feet on the floor of the foot-
                            than 60 cm (2 ft) deep from the bottom of
                                                                     well.
                            the watercraft, otherwise pebbles or sand
                            could be sucked into the jet intake, caus-
                            ing impeller damage and engine overheat-
                            ing.

                                                                  (4) Look  in all directions, start  the  engine,
                                                                     and then start off slowly.
                                                                  EJU44210
                                                                  Capsized watercraft
                                                                  EWJ00672
                            EJU45380
                            Starting off from a trailer
                            (1) Launch the watercraft.            Improper uprighting can cause injury.
                            (2) Attach the engine shut-off cord (lanyard)   Be sure to shut the engine off by pulling
                                to your left wrist, and then attach the clip  on the engine shut-off cord (lanyard) to
                                to the engine shut-off switch.     remove the clip from the engine shut-off
                            (3) Look in all directions, and then start the  switch.
                                engine.                            Do not put your hands in the intake
                            (4) Squeeze the RiDE lever and  move the  grate.
                                watercraft back slowly. (See page 34 for
                                                                  If the watercraft capsizes, turn it over imme-
                                RiDE lever operation procedures.)
                                                                  diately.
                            TIP:                                  To upright the watercraft:
                            When using the RiDE lever to start off from a  (1) Remove the clip from the engine shut-off
                            trailer, you can use the reverse assist to tem-  switch.
                            porarily increase the engine speed. (See page  (2) Swim to the rear of the watercraft. Turn
                            36 for reverse assist operation procedures.)  the watercraft over by pulling on the ride
                            EJU33114                                 plate with one hand while pushing down
                            Boarding and starting off from a dock
                            (1) Board the watercraft from the side.

                            84

| 85 86 87 88 89 90 91 92 93 94 95 |