Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-92
P. 42

    UF4S10E0.book  Page 36  Monday, September 28, 2020  1:50 PM

                            Watercraft operation

                                                                  EJU40003
                            TIP:                                   Watercraft operation modes
                            If the RiDE lever is squeezed while the throttle
                            lever is squeezed, the  watercraft  will  slow  EJU45891
                            down, and once stopped, move in reverse.  Reverse assist
                            To shift into neutral from forward:   The reverse assist is a function for temporar-
                            (1) Release the throttle lever.       ily increasing the engine speed when moving
                            (2) Lightly squeeze and release the RiDE le-  in  reverse,  such as to  enter the water
                                ver. The “N” (neutral) shift indicator will  smoothly when launching the watercraft from
                                be displayed.                     a trailer.
                                                                  This function operates  after the engine is
                                                                  started and only if the watercraft is not shifted
                                                                  into forward.
                                                                  TIP:
                                                                  Once the watercraft is shifted into forward af-
                                                                  ter the engine is started, the reverse assist
                                                                  cannot be operated.
                                                                  Activating and deactivating the reverse
                                                                  assist
                                                                  The activation of the reverse assist can be
                                                                  confirmed by the reverse assist indicator on
                                                                  the multifunction information center.

                                                    MPH
                                                    RPM                                  MPH
                                                                                         RPM
                                                                            Reverse Assist  +2
                              14.3V
                                                           1       14.3V
                              1 “N” (Neutral position)                           1       2
                                                                   1 Reverse assist indicator
                            TIP:
                                                                   2 Reverse assist level
                            If the RiDE lever is squeezed continuously,
                            the reverse gate will move to the reverse po-  To activate the reverse assist:
                            sition.                               (1) Start the engine.
                                                                  (2) Squeeze the RiDE lever to the fully open
                                                                     position, and then push the upper side of
                                                                     the “SPEED ADJUST” switch. Once the
                                                                     beeper sounds three times and the re-
                                                                     verse assist indicator is displayed, the
                                                                     engine speed will  increase. The engine

                            36

| 37 38 39 40 41 42 43 44 45 46 47 |