Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 93 - LIT-18626-12-92
P. 93

    UF4S10E0.book  Page 87  Monday, September 28, 2020  1:50 PM

                                                                           Care and storage

                            EJU37146                              (3) Connect the garden hose  adapter to a
                                   Post-operation care
                                                                     garden hose.
                            EWJ00331

                            Always place the watercraft upright in a      1               2
                            horizontal position when storing it, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which could create
                            a fire hazard.
                            After using the watercraft, always take it out
                            of the water, clean it, and store it. Leaving the
                            watercraft in the water for extended periods
                                                                   1 Garden hose adapter
                            will accelerate the rate of normal deteriora-
                                                                   2 Garden hose
                            tion of the jet pump and hull. Marine organ-
                            isms  and corrosion  are some of the  (4) Loosen the flushing hose connector cap
                            conditions that can shorten the life of many  and  remove  it. Insert the garden  hose
                            watercraft components.                   adapter into the flushing hose connector
                            EJU46120                                 by pushing and twisting it until it is se-
                            Flushing the cooling water passages      curely connected.
                            ECJ01880
                                                                            2
                             Do not run the engine over 4000 r/min on
                              land. Also, do not run  the engine for
                              more than 15 seconds without supplying
                                                                            3                    1
                              water, otherwise the engine could over-
                              heat.
                             Flush the cooling water passages to
                              prevent them from  clogging with salt,
                              sand, or dirt.
                                                                   1 Flushing hose connector cap
                            (1) Place the watercraft in a horizontal posi-
                                                                   2 Garden hose adapter
                                tion.
                                                                   3 Flushing hose connector
                            (2) Remove the seats and  seat  storage
                                                                  (5) Connect the garden hose to a water tap.
                                compartment. (See page 51 for seat re-
                                                                  (6) Make sure that the area around the wa-
                                moval and  installation procedures and
                                                                     tercraft is  clear, and then  start the en-
                                page 56 for information on the seat stor-
                                                                     gine. Immediately after the engine starts,
                                age compartment.)
                                                                     fully turn the water supply on so that wa-

                                                                                                   87

| 88 89 90 91 92 93 94 95 96 97 98 |