Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - LIT-18626-12-92
P. 74

    UF4S10E0.book  Page 68  Monday, September 28, 2020  1:50 PM

                            Pre-operation checks

                            EJU32282                              EJU34215
                               Pre-operation check points         Fuel system checks
                                                                  EWJ00382
                            EJU40099
                            Pre-launch checks
                            Perform the pre-launch checks in the pre-op-  Leaking fuel can result in fire or explosion.
                            eration checklist while the watercraft is  on   Check for fuel leakage regularly.
                            land.                                  If any fuel leakage is found, the fuel sys-
                            To perform the pre-launch checks:      tem must be repaired by a qualified me-
                            (1) Remove the seats and  seat  storage  chanic. Improper repairs can make the
                                compartment. (See page 51 for seat re-  watercraft unsafe to operate.
                                moval and  installation procedures and
                                page 56 for information on the seat stor-  Make sure that there is no damage, leakage,
                                age compartment.)                 or other problem in the fuel system.
                            (2) Perform the checks and make sure that  Check:
                                there are no malfunctioning items or oth-   Fuel filler cap and seal for damage
                                er problems.                       Fuel tank for damage and leakage
                            (3) After completing these checks, securely   Fuel hoses and joints for damage and leak-
                                install the seat storage compartment and  age
                                seats in their original positions.   Fuel tank breather hose  for damage and
                            EJU32334                               leakage
                            Engine compartment check              EJU36875
                            EWJ00462                              Fuel level check
                                                                  Check the fuel level in the fuel tank.
                            Failure  to  ventilate the engine compart-  Add fuel if necessary. (See page 59 for infor-
                            ment could result in a fire or explosion. Do  mation on filling the fuel tank.)
                            not start the engine if there is a fuel leak.  EJU32424
                                                                  Water separator check
                                                                  Make sure that no water has collected in the
                            Ventilate the engine compartment. Leave the
                                                                  water separator. If water has collected in the
                            engine compartment open for a few minutes
                                                                  water separator, drain it. (See page 33 for in-
                            to allow any fuel vapors to escape.
                                                                  formation on draining the water separator.)
                            Make sure that there is no damage inside the
                            engine compartment.

                                                                                                   1

                                                                   1 Water separator

                            68

| 69 70 71 72 73 74 75 76 77 78 79 |