Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-12-92
P. 80

    UF4S10E0.book  Page 74  Monday, September 28, 2020  1:50 PM

                            Pre-operation checks

                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]

                                                    MPH
                                                    RPM
                                                    2
                                                    3
                              14.3V
                                                    4
                                                           1
                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)
                            EJU40172
                            Engine idling speed check
                            Start the engine and warm it up. Use the ta-
                            chometer in the multifunction  information
                            center to make  sure  that the engine  idling
                            speed is not significantly above or below the
                            specified range.

                              Engine idling speed:
                                1300 ±100 r/min

                            74

| 75 76 77 78 79 80 81 82 83 84 85 |