Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 79 - LIT-18626-12-92
P. 79

    UF4S10E0.book  Page 73  Monday, September 28, 2020  1:50 PM

                                                                    Pre-operation checks

                            flood the engine compartment and cause  EJU40146
                                                                  Post-launch checks
                            the watercraft to submerge. [ECJ00363]
                                                                  Perform the post-launch checks in the pre-
                                                                  operation checklist while the watercraft is in
                                                                  the water and the engine is running.
                                                                  To perform the post-launch checks:
                                                                  (1) Launch the watercraft. (See page 76 for
                                                                     information on launching the watercraft.)
                                                                  (2) Perform the checks and make sure that
                                                  2                  there are no malfunctioning items or oth-
                                                                     er problems.
                                                  1               EJU40553
                                                                  Cooling water pilot outlet check
                              1 Stern drain plug                  Make sure that water is discharged from the
                              2 O-ring
                                                                  cooling water pilot outlet while the engine is
                            Securely install the stern drain plugs by tight-  running. (See page 32 for information on the
                            ening them until they stop.           cooling water pilot outlet.)

                                                   1

                              1 Stern drain plug                  EJU45260
                                                                  Multifunction information center check
                            EJU41441
                            Hood check                            Make sure that the multifunction information
                            Push down on the rear of the hood and make  center operates properly. (See page 42 for in-
                            sure that it is securely closed.      formation on proper operation of the multi-
                                                                  function information center.)
                                                                  EJU43393
                                                                  Shift system check
                                                                  Operate the throttle lever and RiDE lever, and
                                                                  check that the watercraft moves or does not
                                                                  move according to the displayed shift indica-
                                                                  tor. (See page 34 for shift system operation
                                                                  procedures.)  WARNING! To avoid colli-
                                                                  sions, operate at safe speeds and keep a

                                                                                                   73

| 74 75 76 77 78 79 80 81 82 83 84 |