Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-12-92
P. 53

    UF4S10E0.book  Page 47  Monday, September 28, 2020  1:50 PM

                                                                     Instrument operation

                            EJU45190                              Fuel” is displayed  on the  display, and  the
                            Engine lock screen “    ”
                                                                  buzzer sounds intermittently.
                            The engine lock screen shows the  setting
                            screen for the Yamaha Security System in the
                            center display. (See page 30 for Yamaha Se-
                            curity System setting procedures.)
                            EJU46400
                            Warning function                                             MPH
                            The multifunction information center can indi-
                                                                                         RPM
                            cate the following warnings.
                             Fuel level warning                                             Low
                                                                                             Fuel
                             Battery voltage warning               14.3V
                             Check engine warning
                             Engine overheat warning             If the fuel level warning is activated, refill the
                             Oil pressure warning                fuel tank as soon as possible. (See page 59
                             Other warnings (communication errors, ex-  for information on filling the fuel tank.)
                              ceeding the maintenance intervals, and so  Battery voltage warning
                              on)                                 If the battery voltage is less than 12 volts or
                            To stop the buzzer when a malfunction is ac-  more than  18  volts when  the engine is not
                            tivated, correct the cause of the problem and  running, the voltage display of the voltmeter
                            start the engine again, or push the “OK” but-  blinks.
                            ton of the touchpad control.

                                                                                         MPH
                                                         1
                                                                                         RPM

                                                                   10.8V

                                                                  If the battery voltage warning  is activated,
                              1 “OK” button
                                                                  have the watercraft  serviced by a  Yamaha
                            Fuel level warning                    dealer as soon as possible.
                            If the amount of remaining fuel is low, the low-  Check engine warning “  ”
                            est fuel level segment blinks orange, “Low  If a sensor  malfunction or a short circuit is
                                                                  detected, “  ” is shown in the warning bar,
                                                                  and the buzzer sounds intermittently.

                                                                                                   47

| 48 49 50 51 52 53 54 55 56 57 58 |