Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 103 - LIT-18626-12-92
P. 103

    UF4S10E0.book  Page 97  Monday, September 28, 2020  1:50 PM

                                                                                Specifications

                            EJU46440                                Spark plug (NGK):
                                      Specifications                  LFR6A
                            Watercraft capacity:                    Spark plug gap:
                              Maximum people on board:                0.8–0.9 mm (0.031–0.035 in)
                                3 person                            Battery capacity:
                              Maximum load capacity:                  12 V, 18 Ah
                                240 kg (530 lb)                     Battery type:
                            Dimensions and weight:                    YTX20L-BS
                              Length:                               Charging system:
                                3.37 m (132.7 in)                     Flywheel magneto
                              Width:                              Drive unit:
                                1.24 m (48.8 in)                    Propulsion system:
                              Height:                                 Jet pump
                                1.20 m (47.2 in)                    Jet pump type:
                              Dry weight:                             Axial flow, single stage
                                352 kg (776 lb) (VX CRUISER HO)     Impeller rotation:
                                360 kg (794 lb) (VX CRUISER HO with audio,   Counterclockwise
                                VX LIMITED HO)                      Jet thrust nozzle angle:
                            Performance:                              24+24 °
                              Maximum fuel consumption:           Fuel and oil:
                                49.7 L/h (13.1 US gal/h, 10.9 Imp.gal/h)  Recommended fuel:
                              Cruising range at full throttle:        Regular unleaded gasoline
                                1.41 hour                           Minimum octane rating (PON):
                              Trolling speed:                         86
                                1300 ±100 r/min                     Minimum octane rating (RON):
                            Engine:                                   90
                              Engine type:                          Recommended engine oil:
                                Liquid cooled 4-stroke, DOHC          YAMALUBE 4W or 4-stroke motor oil
                              Number of cylinders:
                                4
                              Engine displacement:
                                1812 cm³
                              Bore × stroke:                        Recommended engine oil type SAE:
                                86.0 × 78.0 mm (3.39 × 3.07 in)       SAE 10W-30, 10W-40, 20W-40, 20W-50
                              Compression ratio:                    Recommended engine oil grade API:
                                11.0 : 1                              API SG, SH, SJ, SL
                              Valve clearance-intake (cold):        Fuel tank total capacity:
                                0.14–0.23 mm (0.0055–0.0091 in)       70 L (18.5 US gal, 15.4 Imp.gal)
                              Valve clearance-exhaust (cold):       Engine oil quantity with oil filter replacement:
                                0.28–0.37 mm (0.0110–0.0146 in)       3.7 L (3.91 US qt, 3.26 Imp.qt)
                              Lubrication system:                   Engine oil quantity without oil filter replacement:
                                Wet sump                              3.5 L (3.70 US qt, 3.08 Imp.qt)
                              Cooling system:                       Engine oil total quantity:
                                Water                                 5.3 L (5.60 US qt, 4.66 Imp.qt)
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.

                                                                                                   97

| 98 99 100 101 102 103 104 105 106 107 108 |