Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-12-92
P. 45

    UF4S10E0.book  Page 39  Monday, September 28, 2020  1:50 PM

                                                                      Watercraft operation

                                Wake –1”, “No Wake” (standard setting),  drive control mode indicator is shown in light
                                and “No Wake +1”.                 yellow.
                                                                                         1

                                                                              Drive Control

                                                                           Speed/Acceleration

                                                                                 Lock
                                                    1

                              1 “SPEED ADJUST” switch              1 Drive control mode indicator
                            To deactivate the no-wake mode:       To operate the watercraft using the drive con-
                            Perform one of the following operations. The  trol mode:
                            beeper sounds two times and the no-wake  (1) Release the throttle lever and let the en-
                            mode indicator disappears  when the  no-  gine speed return to idle.
                            wake mode is deactivated.             (2) Activate each drive control mode.
                             Push the “CRUISE/NO WAKE” switch.   (3) Squeeze the throttle lever.
                             Squeeze the throttle lever.         Selecting the drive control mode settings
                             Squeeze the RiDE lever.             The drive control mode settings for the maxi-
                            TIP:                                  mum watercraft speed and acceleration are
                                                                  saved. In addition, the activation and settings
                            The no-wake mode is also deactivated when
                                                                  of the drive control mode can be locked to
                            the engine is stopped.
                                                                  prevent others from changing them.
                            EJU46340
                            Drive control mode                    When the drive control mode is locked, a PIN
                            The drive control mode is a function for set-  must be entered to operate the drive control
                            ting the maximum watercraft speed and ac-  mode screen.
                            celeration for stable towing.         To select the maximum watercraft speed and
                            The maximum watercraft speed can be se-  acceleration settings:
                            lected from three settings and the accelera-  (1) Select “Speed/Acceleration”.
                            tion can be selected from two settings.
                            Activating the drive control mode
                            Activation of the drive control mode can be
                            confirmed by the drive control mode indica-
                            tor on  the multifunction information center.
                            When the drive control mode is activated, the

                                                                                                   39

| 40 41 42 43 44 45 46 47 48 49 50 |