Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 68 - LIT-18626-12-92
P. 68

    UF4S10E0.book  Page 62  Monday, September 28, 2020  1:50 PM

                            Operation and handling requirements

                            (3) Remove the dipstick and wipe it clean.  (6) Loosen the engine oil filler cap and re-
                                                                     move it.

                                                      1

                                                                                                1

                              1 Dipstick
                            (4) Insert the dipstick back into the dipstick  1 Engine oil filler cap
                                tube  completely. Remove the  dipstick  (7) Slowly add engine oil.
                                again and make sure that the engine oil  TIP:
                                level is between the minimum and maxi-  The difference between the minimum and
                                mum level marks.                  maximum level marks on the dipstick is equal
                                                                  to approximately 1 L (1.06 US qt, 0.88 Imp.qt)
                                                                  of engine oil.
                                                                  (8) Wait approximately 5 minutes to allow
                                                                     the engine oil to settle, and then check
                                                     1               the engine oil level again.
                                                                  (9) Repeat steps 3–8 until the engine oil is at
                                                     2
                                                                     the proper level.
                                                                  (10) Securely install the engine oil filler cap by
                                                                     tightening it until it stops.
                                                                  (11) Securely install the seats in their original
                              1 Maximum level mark
                                                                     positions.
                              2 Minimum level mark
                            (5) If the  engine oil  level is significantly
                                above the maximum level mark, consult
                                a Yamaha dealer. If the engine oil level is
                                below the minimum level mark, add en-
                                gine oil.

                            62

| 63 64 65 66 67 68 69 70 71 72 73 |