Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 76 - LIT-18626-12-92
P. 76

    UF4S10E0.book  Page 70  Monday, September 28, 2020  1:50 PM

                            Pre-operation checks

                            right and left fully turned positions of the jet  lever returns automatically to its fully closed
                            thrust nozzle.                        position when released.

                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                              Difference between fully turned posi-
                              tions of jet thrust nozzle (distances A
                              and B):
                                Maximum 5 mm (0.20 in)

                            EJU43213
                            RiDE lever checks
                            Operate the RiDE lever several times to make  EJU45351
                            sure that operation is smooth throughout the  Yamaha Security System check
                            whole range. Also, make sure that the RiDE  Make sure that the Yamaha Security System
                                                                  operates properly. (See page 30 for Yamaha
                                                                  Security System setting procedures.)
                                                                  EJU32664
                                                                  Engine shut-off cord (lanyard) check
                                                                  Make sure that the engine shut-off cord (lan-
                                                                  yard) is not damaged. If the cord is damaged,
                                                                  replace it.  WARNING! Never try to repair
                                                                  the engine shut-off cord (lanyard) or tie it
                                                                  together. The  engine  shut-off cord (lan-
                                                                  yard) may not pull free when the operator

                            70

| 71 72 73 74 75 76 77 78 79 80 81 |