Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-92
P. 63

    UF4S10E0.book  Page 57  Monday, September 28, 2020  1:50 PM

                                                                     Equipment operation

                            To close the seat storage compartment:  To use the fire extinguisher holder and cover:
                            (1) Insert the projections on the lid into the  (1) Pull the hood latch rearward, and then lift
                                slots on the seat storage compartment.  up the rear of the hood.

                                                                                                 1

                            (2) Push the rear of the lid down.     1 Hood latch
                                                                  (2) Unhook the band and remove the fire ex-
                                                                     tinguisher from the fire extinguisher cov-
                                                                     er.

                                                                           1

                                                                                               2
                            (3) Securely install the rear seat in its original
                                position.
                            EJU46030
                            Fire extinguisher holder and cover     1 Fire extinguisher holder and cover
                            The fire extinguisher holder and cover are lo-  2 Band
                            cated in the bow storage compartment.
                                                                  (3) Place the fire extinguisher in the fire ex-
                                                                     tinguisher cover, and then securely fas-
                                                                     ten the fire extinguisher with the band.
                                                                  (4) Push the rear of the hood down to se-
                                                                     curely lock it in place. Make sure that the

                                                                                                   57

| 58 59 60 61 62 63 64 65 66 67 68 |