Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-92
P. 44

    UF4S10E0.book  Page 38  Monday, September 28, 2020  1:50 PM

                            Watercraft operation

                            To deactivate the T.D.E.:             Activating and deactivating the no-wake
                            Perform one of the following operations. The  mode
                            T.D.E. indicator disappears and the T.D.E. is  The activation of the no-wake mode can be
                            deactivated.                          confirmed by the no-wake mode indicator on
                             Squeeze the throttle lever.         the multifunction information center.
                             Squeeze the RiDE lever.
                             Push and  hold  the “CRUISE/NO WAKE”
                              switch.
                             While moving forward at a very low speed,                  MPH
                              push the lower side of the “T.D.E.” switch.
                             While moving in reverse at a very low                      RPM
                              speed, push the upper side of the “T.D.E.”       No Wake  +1
                              switch.
                                                                   14.3V
                            TIP:                                                 1    2
                            The T.D.E. is also deactivated when the en-
                                                                   1 No-wake mode indicator
                            gine is stopped.                       2 No-wake mode level
                            EJU45910
                            No-wake mode                          To activate the no-wake mode:
                            The no-wake mode is a function that main-  (1) Shift into neutral, or release the throttle
                            tains the engine speed at a fixed setting for  lever and let the engine speed return to
                            operating the watercraft at low speeds. While  idle.
                            the watercraft is operating in no-wake mode,  (2) Push and hold the “CRUISE/NO WAKE”
                            the engine speed can be adjusted to one en-  switch.  Once  the beeper sounds three
                            gine speed each above and below the initial  times and the no-wake mode indicator is
                            engine speed.                            displayed, the no-wake mode is activat-
                            This function can be used only when the wa-  ed.
                            tercraft is in neutral, or when the watercraft is
                            shifted into forward and the engine is operat-
                            ing at idling speed.
                            TIP:
                            If the no-wake mode is activated when the
                            watercraft is in neutral, the watercraft will au-
                            tomatically shift into forward and the water-
                            craft will start moving at a low speed.
                                                                                              1

                                                                   1 “CRUISE/NO WAKE” switch
                                                                  (3) Push the upper side or the lower side of
                                                                     the “SPEED  ADJUST” switch  to adjust
                                                                     the engine speed to three settings: “No

                            38

| 39 40 41 42 43 44 45 46 47 48 49 |