Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 106 - LIT-18626-12-93
P. 106

    UF4N10E0.book  Page 99  Tuesday, September 29, 2020  8:02 AM

                            Care and storage

                                ter flows out continually from  the  jet  (See page 102 for information on rust-
                                thrust nozzle.                       proofing the  internal engine  compo-
                                                                     nents.)
                                                                  (3) Rinse  the engine and engine compart-
                                                                     ment with a small amount of  water.
                                                                     NOTICE: Do not use high-pressure
                                                                     water when rinsing the engine or en-
                                                                     gine  compartment as severe engine
                                                                     damage could result. [ECJ00572]
                                                                  (4) Drain  the water  from the engine com-
                                                                     partment. (See page 72 for information
                                                                     on draining the bilge water.)
                            (7) Run the engine at idling speed for about  (5) Wipe  the engine  and engine compart-
                                3 minutes watching the engine condition.  ment with a dry cloth.
                                If the  engine stops  while flushing,  turn  (6) Wash down the hull, deck, and jet pump
                                the water supply off immediately  and  with fresh water.
                                perform the procedure again from step 6.  (7) Wipe the hull, deck, and jet pump with a
                                NOTICE: Do not supply water to the   dry cloth.
                                cooling water passages when the en-  (8) Wipe  all vinyl and rubber components,
                                gine is not running. The water could  such as the seats and engine compart-
                                flow back through the muffler into the  ment seals, with a vinyl protectant such
                                engine, causing severe engine  dam-  as Yamaclean Vinyl Dressing™.
                                                                  (9) To minimize corrosion, spray metallic
                                age. [ECJ00123]
                            (8) Turn the water supply off.           parts of the hull, deck, and engine with a
                            (9) Discharge the remaining water out of the  rust inhibitor such as Yamalube Silicone
                                cooling  water passages by  alternately  Protectant & Lubricant.
                                squeezing and releasing the throttle lever  (10) Allow the engine compartment to air dry
                                quickly for 10 to 15 seconds.        completely before installing the seats.
                            (10) Stop the engine.                 (11) Securely install the seats in their original
                            (11) Remove the garden hose adapter, and  positions.
                                then securely install the flushing hose  EJU41635
                                                                  Battery care
                                connector cap  by tightening  it until it
                                                                  If the watercraft will not be used for more than
                                stops.
                                                                  a month, remove the battery from the water-
                            (12) Securely install seats in their original po-
                                                                  craft, check it, and then store it in a cool, dry
                                sitions.
                                                                  place.
                            EJU43931
                            Cleaning the watercraft               EWJ00793
                            (1) Remove the seats. (See page 60 for seat
                                removal and installation procedures.)  Battery electrolyte is poisonous and dan-
                            (2) If the watercraft will be stored for a week  gerous, causing severe burns, etc. Elec-
                                or more,  rustproof  the internal engine  trolyte contains sulfuric acid. Avoid
                                components to help prevent corrosion.  contact with skin, eyes, or clothing.

                            99

| 101 102 103 104 105 106 107 108 109 110 111 |