Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-93
P. 39

    UF4N10E0.book  Page 32  Tuesday, September 29, 2020  8:02 AM

                                                             Control function operation

                            EJU31154                              start/stop switch, wait 15 seconds, and then
                            Engine stop switch “ ” (VX-C)
                                                                  try again.
                            The engine stop switch (red button) stops the
                            engine when the switch is pushed.

                                                                                      1

                                                       1           1 Engine start/stop switch
                                                                  The engine will not start under any of the fol-
                              1 Engine stop switch
                                                                  lowing conditions:
                            EJU46112
                            Engine start/stop switch “  / ” (VX /    VX DELUXE / VX CRUISER / VX LIMITED:
                            VX DELUXE / VX CRUISER / VX            Lock mode of the Yamaha Security System
                            LIMITED)                               has been selected. (See page 31 for
                                                                   Yamaha Security System setting proce-
                            ECJ01311
                                                                   dures.)
                            Do not run the engine over 4000 r/min on   Clip is removed from the engine shut-off
                            land. Also, do not run the engine for more  switch.
                            than 15 seconds without supplying water,   Throttle lever is squeezed.
                            otherwise the engine could overheat.   Throttle lever is malfunctioning.
                                                                   RiDE lever is squeezed.
                            The  engine start/stop switch  (red button)
                                                                   RiDE lever is malfunctioning.
                            starts the engine when the switch is pushed
                                                                  EJU31164
                            while the engine is stopped, and stops the  Engine shut-off switch “  ”
                            engine when the switch is pushed while the  The engine  shut-off switch  automatically
                            engine is running.                    stops the engine when the clip, on the end of
                            Release the engine start/stop switch as soon  the engine shut-off cord (lanyard), is removed
                            as the engine starts to run. If the engine does  from the switch, such as if the operator falls
                            not start in 5 seconds, release the engine  off the watercraft.

                                                                                                   32

| 34 35 36 37 38 39 40 41 42 43 44 |